|  |  |
| --- | --- |
| **Question** | **Answer** |
| In order to select the correct drilling rig equipment, please provide the dimensions of the explosion hazard zones for XYZ axles (Explosion hazardous Areas) according to the ATEX directive | Explosion zone of Inčukalns UGS wells: 2.5 m (spherical radius) - zone 1,4m (spherical radius) - zone 2.work environment - natural gas (methane).Explosive equipment in a workover rig must comply with the technical specification p.1 |