|  |  |
| --- | --- |
| **Question** | **Answer** |
| In order to select the correct drilling rig equipment, please provide the dimensions of the explosion hazard zones for XYZ axles (Explosion hazardous Areas) according to the ATEX directive | Explosion zone of Inčukalns UGS wells:   2.5 m (spherical radius) - zone 1,  4m (spherical radius) - zone 2.  work environment - natural gas (methane).  Explosive equipment in a workover rig must comply with the technical specification p.1 |