**26.09.2019.**

**Question:** In technical Requirements Appendix No.1 well №124 diameter of Production casing is given **-** 152,4 мм. – is it correct?

**Answer:** Production casing of wells No. 124, 133, 135, 140 - 6⅝", which corresponds to 168 (168,3) mm.

**Question:** Contest regulation sub-clause (p.5.2.5.3.) is stated after the day when the successful Tenderer submits the Contract Performance security in amount of 5% (five per cent) of the Contract price, but in the draft contract requires Contract performance 3% (p. 4)?

**Answer:** According to Contract project ( Clause 4.1.) and Form of Tender letter (Clause 8.), Contract Performance security in sub-clause 5.2.5.3. should be in amount of 3%. Technical corrections will be made in Regulation.